


Details about Bluetooth Serial Transceiver Module Base Board clear button For Arduino SWTG

*Description:*

* Commercial Series: Bluetooth module board Series
* With LED indicator light, use 150mA and 3.3V regulation chip.
* With VCC、GND、TXD、RXD foot for the Bluetooth.
* With "Re-seach" button(ON/OFF/WAKE foot for it , external MCU outinput "High level" can control module to re-seach).
* Compatible with bluetooth master module"、slave module"or master-slave(whole) module.
* Input voltage: 3.3~6V.
* Size: 1.55cm\*3.98cm.

*Note:*

* Input power supply 3.3~6V, Prohibit more than 7V
* No "Automatically prevent power supply peversing func", so please correctly connect power supply
* We advise to install "Bluetooth master module"
* The "State" is output foot for LED status, when bluetooth "Unconnected", output "Pulse" ; when bluetooth "connected", output "High level", we can determine the states from "MCU"
* If only the board , No any "Bluetooth Function "



*Package Included:*

* 1PCS\*Bluetooth Serial Transceiver Module Base Board Enable clear button For Arduino