SV3C 960p Security Camera sv-b01 - Connection Drops Out Frequently using ISPY

After reducing the “Maximum Frame Rate” I had problems with connectivity with this camera. I normally scan this camera at 1 fps. In this case increasing the “Maximum FrameRate” to 10 fixed the problem.

Increase the “Maximum Frame Rate” under “Setting, Video Setting, Maximum Frame Rate using the “Searchtool” software provided with the unit.