**1602 LCD Board Keypad Shield Blue Backlight for Arduino Duemilanove Robot**

Product Details: 1602 LCD Board Keypad Shield

Condition: New

Dimension: 8 x 5.9cm

This is a basic 16 character by 2 line black-on-green display

Utilizes the extremely common HD44780 parallel interface chipset

Interface code is freely available

Blue Backlight with white words

Uses 4 Bit Arduino LCD Library

Color and more details are shown as pictures

PLS NOTE that due to lighting effects, monitor's brightness/ contrass settings ect, there could be some slight differences in the color tone of the pictures and the actual item!