**2 in one SD Card and TF Card Arduino Shield for Arduino UNO R3 Arduino Mega 2560**

**2 in one SD Card and TF Card Arduino Shield for Arduino UNO R3 Arduino Mega 2560**

**Overview:**

This SD card shield is a standard SD card / TF card break out board for Arduino. The SD card shield adds storage to your Arduino project. It supports SD, SDHC, or Micro SD/TF cards. It just uses the SPI ports of Arduino, and you can plug more other shield on it.

**Features:**

Arduino compatible

SD card, Micro SD card and SDHC card supportable

Prototype expand

Arduino Library support

Size: 53mm x 47mm

Weight: 35g

| Pin of Arduino | With SD Card |
| --- | --- |
| 5V | VCC à 3v3 |
| GND | GND |
| D13 | SD\_CLK |
| D12 | SD\_OUT |
| D11 | SD\_IN |
| D10 | SD\_CS |

**Package Include:**

1\* SD/TF Card 2 in one Arduino Shield module







