

# **HMC5883L Triple Axis Magnetometer Compass Sensor Module 3V-5V For Arduino**

Features:

* Brand new and high quality.
* HMC5883L module (three-axis magnetic field module).
* Use the chip: HMC5883L.
* Power supply: 3-5V.
* Communication modes: standard IIC communication protocol.
* Measuring range: ± 1.3-8 Gauss.
* Size: 1.5cm x 1.8cm.

Package Included:

* 1 x HMC5883L Compass Magnetometer Sensor Module

<http://www.uctronics.com/download/U3071-HMC5883L.zip>